EXP 3 :Write an assembly language program for adding two 16-bit data using 8085 processor?

LDA 1000

MOV B,A

LDA 1001

MOV C,A

LDA 1002

MOV D,A

LDA 1003

ADD C

STA 1005

MOV A,D

ADD B

STA 1004

HLT

